**GJ5606- DuoDrive - Motor for Venetian blinds**

**Motor**

230V / 50Hz motor for concealed installation, torque: 6 Nm, speed: 9 revolutions per minute for the rotation of the slats and 39 revolutions per minute for the blind movements,

IP 54, integrated, multi-stage planetary gear with change of direction after a 3/4 rotation and two-sided shaft, built-in limit stop switch, capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free.

The motor must be installed with a noise-optimized damping to reduce the borne sound transmission to a minimum.

Upper and lower limit stops are freely adjustable. Optional shutdown in the upper end position by means of the limit stop switch without any further setting. The DuoDrive has two different speeds.