**GJ56.. Motor for Venetian blinds**

**Motor**

230V / 50Hz motor for concealed installation, torque: 6, 10, 16 or 20 Nm according to type,

speed: 26 r / min, IP 54, with integrated, multi-stage planetary gear and two-sided shaft, built-in limit stop switch, capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free.

The motor must be installed with a noise-optimized damping to reduce the borne sound transmission to a minimum.

Upper and lower limit stops are freely adjustable. Optional shutdown in the upper end position by means of the limit stop switch without any further setting.