**SOLIDline Sun AIR – Smart Home Ready**

**Motor**

230V / 50Hz electronic tubular motor for concealed installation, torque: 10, 20, 30, 40,

50 Nm according to type, speed: 16 r / min (with 50 Nm 12 r/min), IP 44, with integrated, multi-stage planetary gear, mounted capacitor and thermal overload protector. Pluggable connection cable. The motor is permanently lubricated and maintenance-free. Several motors can be connected in parallel. Integrated bidirectional radio module AIR.

**Application**: cassette awnings, screens (ZIP screens, facade awnings etc.)

The upper end position is always switched off by torque. This ensures that the cassette is always securely closed. The lower end position can be freely adjusted. Compatible with the LOXONE Smart Home control system.